|  |  |
| --- | --- |
| **Article no.** | **KCR4S2NC0** |
| Model Name: | miscea KITCHEN Standard for Bottle (without water flow regulator) |
|  |  |
| **General** |  |
| Faucet mount type: | Deck mount |
| Soapbox type: | Soapbox for use with bottle |
| Adapter: | 2 pin EU |
| Language display: | N/A |
| Description: | Touch free, electronically controlled kitchen water faucet with two integrated liquid dispensers. |
|  |  |
| **Finish** | Polished chrome finish |
|  |  |
| **Technical Specifications** |  |
| Voltage: | 24 V |
| Input Voltage: | 100 – 240 VAC / 50 – 60 Hz |
| Operating water pressure: | 0.5 to 8 bar |
| Max water temperature: | 70 °C |
| IP rating of PCB: | IP 55 |
|  |  |
| **Features** | Standard miscea KITCHEN faucet - Electronic faucet with 3 selectable fluid options  Faucet user interface made of high quality laser engraved glass  LED display for temperature feedback  Automatic flushing for prevention of waterborne bacteria. Cycles completely adjustable via the miscea remote control (sold separately).  Touch free water temperature controls  2 rotate angles - set during installation |
|  |  |
| **Scope of delivery** | Standard miscea KITCHEN faucet in polished chrome finish  Waterbox component - houses the electronics and solenoid valve.  Soapbox component for use with bottle refills  2 x 84 cm stainless steel braided hoses for hot and cold water connections  2 pin EU power plug  Installation/mounting kit  Instruction manual |
|  |  |
|  |  |