|  |  |
| --- | --- |
| **Article no.** | **CCR3S2NCEN** |
| Model Name: | miscea CLASSIC Wall for Bottle |
|  |  |
| **General** |  |
| Faucet mount type: | Wall mount |
| Soapbox type: | Soapbox for use with bottles |
| Adapter: | 2 pin EU |
| Language display: | English |
| Description: | Touch free, electronically controlled water faucet with integrated soap and disinfectant dispensers. |
|  |  |
| **Finish** | Polished chrome finish |
|  |  |
| **Technical Specifications** |  |
| Voltage: | 24 V |
| Input Voltage: | 100 – 240 VAC / 50 – 60 Hz |
| Operating water pressure: | 0.5 to 8 bar |
| Max water temperature: | 70 °C |
| IP rating of PCB: | IP 55 |
|  |  |
| **Features** | Wall miscea CLASSIC faucet - Electronic faucet with 3 selectable fluid options  Faucet user interface made of high quality laser engraved glass  LED display for temperature feedback  Automatic flushing for prevention of waterborne bacteria. Cycles completely adjustable via the miscea remote control (sold separately).  Touch free water temperature controls  Activation of ‘+’ and ‘-’ sectors at the same time to start Bucket-Fill mode function |
|  |  |
| **Scope of delivery** | Wall miscea CLASSIC faucet  Waterbox component - houses the electronics and solenoid valve.  Soapbox component for use with bottles  2 x 84 cm stainless steel braided hoses for hot and cold water connections  2 pin EU power plug  Installation/mounting kit  Instruction manual |
|  |  |
|  |  |