|  |  |
| --- | --- |
| **Article no.** | **CCR3S1NC** |
| Model Name: | miscea CLASSIC Pure S Wall for Pouches |
|  |  |
| **General** |  |
| Faucet mount type: | Wall mount |
| Soapbox type: | Soapbox for use with pouches |
| Adapter: | 2 pin EU |
| Language display: | - |
| Description: | Touch free, electronically controlled water faucet with integrated soap dispenser. |
|  |  |
| **Finish** | Polished chrome finish |
|  |  |
| **Technical Specifications** |  |
| Voltage: | 24 V |
| Input Voltage: | 100 – 240 VAC / 50 – 60 Hz |
| Operating water pressure: | 0.5 to 8 bar |
| Max water temperature: | 70 °C |
| IP rating of PCB: | IP 55 |
|  |  |
| **Features** | Wall miscea CLASSIC Pure S faucet - Electronic faucet with soap dispenser  Faucet user interface made of high quality laser engraved glass  LED display for temperature feedback  Automatic flushing for prevention of waterborne bacteria. Cycles completely adjustable via the miscea remote control (sold separately).  Touch free water temperature controls  Activation of ‘+’ and ‘-’ sectors at the same time to start Bucket-Fill mode function |
|  |  |
| **Scope of delivery** | Wall miscea CLASSIC Pure S faucet  Waterbox component - houses the electronics and solenoid valve.  Soapbox component for use with pouches  2 x 84 cm stainless steel braided hoses for hot and cold water connections  2 pin EU power plug  Installation/mounting kit  Instruction manual |
|  |  |
|  |  |