|  |  |
| --- | --- |
| **Article no.** | **CER2NC** |
| Model Name: | miscea CLASSIC Pure W Small |
|  |  |
| **General** |  |
| Faucet mount type: | Deck mount |
| Soapbox type: | - |
| Adapter: | 2 pin EU |
| Language display: | - |
| Description: | Touch free, electronically controlled water faucet. |
|  |  |
| **Finish** | Stainless steel finish |
|  |  |
| **Technical Specifications** |  |
| Voltage: | 24 V |
| Input Voltage: | 100 – 240 VAC / 50 – 60 Hz |
| Operating water pressure: | 0.5 to 8 bar |
| Max water temperature: | 70 °C |
| IP rating of PCB: | IP 55 |
|  |  |
| **Features** | Small miscea CLASSIC Pure W faucet - Electronic faucet  Faucet user interface made of high quality laser engraved glass  LED display for temperature feedback  Automatic flushing for prevention of waterborne bacteria. Cycles completely adjustable via the miscea remote control (sold separately).  Touch free water temperature controls |
|  |  |
| **Scope of delivery** | Small miscea CLASSIC Pure W faucet  Waterbox component - houses the electronics and solenoid valve.  2 x 84 cm stainless steel braided hoses for hot and cold water connections  2 pin EU power plug  Installation/mounting kit  Instruction manual |
|  |  |