|  |  |
| --- | --- |
| **Article no.** | **LCR3S1-1NCDE** |
| Model Name: | miscea LIGHT Wall with integrated Soap Dispenser |
|  |  |
| **General** |  |
| Faucet mount type: | Wall mount |
| Soapbox type: | Soapbox for use with 1L miscea vacuum pouch |
| Adapter: | 2 pin EU |
| Language display: | German |
| Description: | Touch free, electronically controlled water faucet with integrated soap dispenser. |
|  |  |
| **Finish** | Polished chrome finish |
|  |  |
| **Technical Specifications** |  |
| Voltage: | 12 V |
| Input Voltage: | 100 – 240 VAC / 50 – 60 Hz |
| Operating water pressure: | 0.8 to 10 bar |
| Max water temperature: | 75 °C |
| IP rating of PCB: | IP 55 |
|  |  |
| **Features** | Wall miscea LIGHT faucet with integrated soap dispenser – Electronic faucet with water and soap option.  User interface made of durable Makrolon (UI)  Pulsing LED light on faucet indicates system is ready for use  Automatic flushing for prevention of waterborne bacteria. Cycles completely adjustable via the miscea remote control (sold separately).  Electronics and solenoid valve designed into faucet  Waterbox not required due to compact design |
|  |  |
| **Scope of delivery** | Wall miscea LIGHT faucet with water and soap dispenser  Soapbox component for use with pouch refills  System must be used with 2 pouches  Liquid refill products not included. Please order separately  1 x 84 cm stainless steel braided hose for water connection  Installation kit  Instruction manual |
|  |  |
|  |  |